/** 
* @file:   README
* CVS:     $Id$
* @author: Dan Terpstra
*          terpstra@icl.utk.edu
* @defgroup papi_components Components
* @brief Component Specific Readme file: BGPM
*/

/** @page component_readme Component Readme 

@section Component Specific Information

bgpm/
Five new components have been added to PAPI to support hardware performance monitoring for the BG/Q platform; in particular the BG/Q network, the I/O system, the Compute Node Kernel in addition to the processing core. There are no specific component configure scripts for L2unit, IOunit, NWunit, CNKunit. In order to configure PAPI for BG/Q, use the following configure options at the papi/src level:
    % ./configure --prefix=< your_choice >  \
                  --with-OS=bgq  \
                  --with-bgpm_installdir=/bgsys/drivers/ppcfloor  \
                  CC=/bgsys/drivers/ppcfloor/gnu-linux/bin/powerpc64-bgq-linux-gcc  \
                  F77=/bgsys/drivers/ppcfloor/gnu-linux/bin/powerpc64-bgq-linux-gfortran  \
                  --with-components="bgpm/L2unit bgpm/CNKunit bgpm/IOunit bgpm/NWunit"

*/
